1. Power on JACO
2. Open Joy2Key
3. Open SDK (check if robot is connected)
4. Open Robotiq software
5. Click on “Control the Gripper using an Xbox Joystick” (in Robotiq software)
6. Activate Keyboard Control (in SDK)
7. Home Robot
8. Do demo